Kawasaki KLX 250s specifications

* Engine: Four-stroke, Liquid-Cooled, DOHC, four-valve single
* Displacement: 249cc
* Bore x Stroke 72.0 x 61.2mm
* Compression ratio 11.0:1
* Cooling System Liquid
* Carburetion Keihin CVK34
* Ignition Digital CDI
* Transmission Six-speed
* Final drive Chain
* Frame Type Semi-double cradle, high-tensile steel
* Rake/Trail 26.5 degrees / 4.1 in.
* Front suspension / wheel travel 43mm inverted cartridge fork with 16-way compression damping adjustment / 10.0 in.
* Rear suspension / wheel travel Uni-Trak® with adjustable preload, 16-way compression and

rebound damping adjustment / 9.1 in.

* Front Tire Size 80/100x21
* Rear Tire Size 100/100x18
* Front brakes / rear brakes 250mm semi-floating petal disc with two-piston hydraulic caliper /

240mm petal disc with single-piston hydraulic caliper

* Overall length 86.6 in.
* Overall width 32.3 in.
* Overall Height 47.4 in.
* Seat height 35.0 in.
* Wheelbase 56.3 in.
* Ground clearance 11.2 in.
* Fuel capacity 2.0 gal.
* Curb weight 297.7 lbs.